**B. Implementation of digital anti-aliasing filters on a DSP**

**b)** Write a c-program which generates two sequences of 256 samples of x(t), using the sampling frequencies F1 = 1.2Hz and F2 = 4.8Hz.

To predict how the signal beh